{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["VBA Script"],"not_rendered":{"charts":4,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"VBA Script","index":0,"n_rows":22,"n_cols":3,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["Given","Values","Units"]
["Compressor type","Lube Injected"]
["Ambient Pressure",14.7,"PSIA"]
["Ambient Temperature",90,"F"]
["Capacity",2977.712,"cfm"]
["Inlet Oil Temperature",90,"F"]
["Inlet Air Pressure",14.3,"PSIA"]
["Max rated Pressure",145.9,"PSIG"]
["Rated power w/ SF",550,"HP"]
["Exit Oil Temp",95,"F"]
["Exit Air Temp",99,"F"]
["Motor Efficiency",0.95]
[]
["Output"]
["Pressure",145.90008876306064,"PSIG"]
["Flow Rate",277.01712968760398,"cfm"]
["Air Temperature Out",98.998795828227259,"F"]
["Oil Temp",95.000072487577256,"F"]
["motor Power",549.88109940927677,"HP"]
["Heat Output",596.76182110749892,"HP"]
["Screw Efficiency",0.912109375]
["Total isothermal Eff",0.83022816591412196]